{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","操作手順"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":6,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"オリンパス　カメラ GPS Log(NMEA形式)　⇒　平面直角座標(XY) 表作成"]
[]
[null,null,null,null,"平面直角座標系",7]
[]
[]
[null,"日時","緯度","経度","X座標","Y座標"]

{"sheet":"操作手順","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
[null,"操作手順"]
[]
[null,"・オリンパス　タフカメラのログデータを取り出す(xx.log)。"]
[null,"・平面直角座標系を選択する。"]
[null,"・ログファイル選択ボタンを押す。"]
[null,"・ログファイルに記録されている日時、緯度、経度、緯度経度から計算した平面直角座標XYが表示される。"]
[]
[null,"注）　AutoCADのXYと平面直角座標のXYのは逆になっている。"]
[]
[]
[null,"参考)国土地理院分かりやすい平面直角座標系"]
[null,"https://www.gsi.go.jp/sokuchikijun/jpc.html"]